<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<library>
<packages>
<package name="MSOP10">
<description>&lt;b&gt;10 Lead Platic MSOP&lt;/b&gt;&lt;p&gt;
Source: http://www.linear.com .. LT1996</description>
</package>
<package name="TSOP-5">
</package>
<package name="SSOP20">
</package>
<package name="MICRO-SD-SOCKET">
</package>
<package name="LGA14">
</package>
<package name="IR_TFDU4300_FOOT">
</package>
<package name="SOIC8">
</package>
<package name="SC70-6">
</package>
<package name="SOIC16">
</package>
<package name="DIP08">
</package>
<package name="DIL08">
</package>
<package name="TO92">
</package>
<package name="SOT23">
</package>
<package name="LED_TH_7.6MM">
</package>
<package name="POT_TYCO_S50">
</package>
<package name="DIL14">
</package>
<package name="HSOP25">
<description>&lt;b&gt;HSOP 25&lt;/b&gt;&lt;p&gt;
Source: http://www.rohm.com/products/databook/motor/pdf/bd623x_series-e.pdf</description>
</package>
<package name="SOT23-6">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; 6 lead</description>
</package>
<package name="D2PACK">
<description>&lt;b&gt;D2PACK&lt;/b&gt;&lt;p&gt;
Source: INTERNATIONAL RECTIFIER, irg4bc15ud-s.pdf</description>
</package>
<package name="PINH1X03">
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="PANASONIC_A">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package A&lt;/b&gt;</description>
</package>
<package name="PANASONIC_B">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package B&lt;/b&gt;</description>
</package>
<package name="PANASONIC_C">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package C&lt;/b&gt;</description>
</package>
<package name="PANASONIC_D">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package D&lt;/b&gt;</description>
</package>
<package name="PANASONIC_E">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package E&lt;/b&gt;</description>
</package>
<package name="PANASONIC_F">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package F&lt;/b&gt;</description>
</package>
<package name="PANASONIC_G">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package G&lt;/b&gt;</description>
</package>
<package name="SO-08">
<description>&lt;B&gt;Small Outline Narrow Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
150-mil body, package type SN</description>
</package>
<package name="CIID-LOGO">
</package>
<package name="CIID-LABS-LOGO">
</package>
<package name="SOT25">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;&lt;p&gt;
TSC [Taiwan Semiconductor Company, Ltd]&lt;br&gt;
Source: http://www.taiwansemi.com .. 5205_0409c.pdf</description>
</package>
<package name="CIID-LABS-LOGO-SMALL">
</package>
<package name="BODYSWITCH">
</package>
<package name="VSIONHAIR">
</package>
</packages>
<symbols>
<symbol name="LTC4053">
<pin name="!CHRG" direction="out"/>
<pin name="NTC" direction="in"/>
<pin name="TIMER"/>
<pin name="GND" direction="pwr"/>
<pin name="PROG"/>
<pin name="BAT" direction="pwr"/>
<pin name="!FAULT" direction="out"/>
<pin name="!ACPR" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="!SHDN" direction="in"/>
</symbol>
<symbol name="NCP1450A">
<pin name="!CE" direction="in"/>
<pin name="OUT" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="EXT"/>
</symbol>
<symbol name="SSOP20">
</symbol>
<symbol name="QT240">
<pin name="SNS2"/>
<pin name="SNS2K"/>
<pin name="SNS1"/>
<pin name="SNS1K"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
<pin name="SYNC/SS"/>
<pin name="NC0" direction="nc"/>
<pin name="NC1" direction="nc"/>
<pin name="VSS" direction="pwr"/>
<pin name="!RES" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="OSC"/>
<pin name="NC2" direction="nc"/>
<pin name="SNS4"/>
<pin name="SNS4K"/>
<pin name="SNS3"/>
<pin name="SNS3K"/>
</symbol>
<symbol name="SD-MMC">
<pin name="DAT2"/>
<pin name="CD/DAT3"/>
<pin name="CMD"/>
<pin name="VSS1"/>
<pin name="VDD"/>
<pin name="DAT1"/>
<pin name="DAT0"/>
<pin name="VSS2"/>
<pin name="CLK"/>
</symbol>
<symbol name="MMA7341L">
<pin name="XOUT" direction="out"/>
<pin name="YOUT" direction="out"/>
<pin name="ZOUT" direction="out"/>
<pin name="GSEL" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="TEST"/>
<pin name="!SLEEP" direction="in"/>
</symbol>
<symbol name="TFDU4300">
<pin name="IREDA"/>
<pin name="IREDC"/>
<pin name="TXD"/>
<pin name="RXD"/>
<pin name="SD"/>
<pin name="VCC"/>
<pin name="VLOGIC"/>
<pin name="GND"/>
</symbol>
<symbol name="QT320">
<pin name="S1A"/>
<pin name="S1B"/>
<pin name="S2A"/>
<pin name="S2B"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT1" direction="out"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="LM4893">
<pin name="!SHUT" direction="in"/>
<pin name="BYPASS"/>
<pin name="IN+"/>
<pin name="IN-"/>
<pin name="VO1"/>
<pin name="VO2"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="OPAMP+-">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="LTC2630">
<pin name="!CS/LD" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="VOUT"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="MICRF0XX">
<pin name="SEL0"/>
<pin name="VSSRF1"/>
<pin name="VSSRF2"/>
<pin name="ANT"/>
<pin name="VDDRF"/>
<pin name="VDDBB"/>
<pin name="CTH"/>
<pin name="NC"/>
<pin name="VSSBB"/>
<pin name="DO"/>
<pin name="SHUT"/>
<pin name="WAKEB"/>
<pin name="CAGC"/>
<pin name="SEL1"/>
<pin name="REFOSC"/>
<pin name="SWEN"/>
</symbol>
<symbol name="SN75176A">
<pin name="R" direction="in"/>
<pin name="!RE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="D" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="A"/>
<pin name="B"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="SN75178">
<pin name="!EN" direction="in"/>
<pin name="A"/>
<pin name="B"/>
<pin name="T"/>
<pin name="Z"/>
<pin name="Y"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="LM380N-8">
<pin name="NC" direction="nc"/>
<pin name="+"/>
<pin name="-"/>
<pin name="GND" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="VOUT" direction="out"/>
<pin name="VS" direction="pas"/>
<pin name="BP" direction="pas"/>
</symbol>
<symbol name="MCP4921">
<pin name="VDD" direction="pwr"/>
<pin name="!CS" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="!LDAC" direction="in"/>
<pin name="VREF" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="VOUT" direction="pas"/>
</symbol>
<symbol name="MCP120/130">
<pin name="VDD" direction="in"/>
<pin name="!RST" direction="out"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="LED_RGB">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="A2" direction="pas"/>
</symbol>
<symbol name="POT">
<pin name="A" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="74HCT32N">
<pin name="1A" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="1Y" direction="out"/>
<pin name="2A" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2Y" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="3Y" direction="out"/>
<pin name="3A" direction="in"/>
<pin name="3B" direction="in"/>
<pin name="4Y" direction="out"/>
<pin name="4A" direction="in"/>
<pin name="4B" direction="in"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="OPAMP+-8">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="BYPASS" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="G2" direction="pas"/>
<pin name="V-" direction="pwr"/>
<pin name="G1" direction="pas"/>
<pin name="V+" direction="pwr"/>
</symbol>
<symbol name="BD622XFP">
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="VCC@4" direction="pwr"/>
<pin name="OUT1A"/>
<pin name="OUT2A"/>
<pin name="RNFA"/>
<pin name="OUT1B"/>
<pin name="OUT2B"/>
<pin name="RNFB"/>
<pin name="VREFA" direction="pwr"/>
<pin name="FINA"/>
<pin name="RINA"/>
<pin name="VREFB" direction="pwr"/>
<pin name="FINB"/>
<pin name="RINB"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="SWITCH-SPDT">
<pin name="OUT" direction="pas"/>
<pin name="INB" direction="pas"/>
<pin name="INA" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="VCC2">
<pin name="VCC" direction="sup"/>
</symbol>
<symbol name="DUAL-OPAMP+-">
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="OUTA" direction="out"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="PWR+GND">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="VREG-3PINS">
<pin name="IN" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="OUT" direction="pas"/>
</symbol>
<symbol name="OPAM+-GGBP">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="BYPASS" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="G2" direction="pas"/>
<pin name="V-" direction="pwr"/>
<pin name="G1" direction="pas"/>
<pin name="V+" direction="pwr"/>
</symbol>
<symbol name="MCP73831">
<pin name="VDD" direction="pwr"/>
<pin name="STAT"/>
<pin name="VBAT" direction="pas"/>
<pin name="PROG"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="LTC3407">
<pin name="VFB2"/>
<pin name="SW2"/>
<pin name="MODE"/>
<pin name="RUN2"/>
<pin name="VIN" direction="pwr"/>
<pin name="RUN1"/>
<pin name="!RESET"/>
<pin name="SW1"/>
<pin name="VFB1"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="MCP1640">
<pin name="VIN" direction="pwr"/>
<pin name="EN"/>
<pin name="GND" direction="pwr"/>
<pin name="VFB"/>
<pin name="VOUT" direction="pwr"/>
<pin name="SW"/>
</symbol>
<symbol name="CIID-LABS">
</symbol>
<symbol name="BODYSWITCH">
<pin name="A"/>
<pin name="B"/>
</symbol>
<symbol name="VSIONHAIR">
</symbol>
</symbols>
<devicesets>
<deviceset name="LTC4053EMSE-4.2">
<description>USB Compatible
Lithium-Ion Battery Charger
with Thermal Regulation</description>
<gates>
<gate name="G$1" symbol="LTC4053"/>
</gates>
<devices>
<device name="" package="MSOP10">
<connects>
<connect gate="G$1" pin="!ACPR" pad="10"/>
<connect gate="G$1" pin="!CHRG" pad="1"/>
<connect gate="G$1" pin="!FAULT" pad="3"/>
<connect gate="G$1" pin="!SHDN" pad="8"/>
<connect gate="G$1" pin="BAT" pad="9"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="NTC" pad="6"/>
<connect gate="G$1" pin="PROG" pad="7"/>
<connect gate="G$1" pin="TIMER" pad="4"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP1450A">
<gates>
<gate name="G$1" symbol="NCP1450A"/>
</gates>
<devices>
<device name="" package="TSOP-5">
<connects>
<connect gate="G$1" pin="!CE" pad="1"/>
<connect gate="G$1" pin="EXT" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="QT240">
<gates>
<gate name="G$1" symbol="QT240"/>
</gates>
<devices>
<device name="" package="SSOP20">
<connects>
<connect gate="G$1" pin="!RES" pad="13"/>
<connect gate="G$1" pin="NC0" pad="10"/>
<connect gate="G$1" pin="NC1" pad="11"/>
<connect gate="G$1" pin="NC2" pad="16"/>
<connect gate="G$1" pin="OSC" pad="15"/>
<connect gate="G$1" pin="OUT1" pad="5"/>
<connect gate="G$1" pin="OUT2" pad="6"/>
<connect gate="G$1" pin="OUT3" pad="7"/>
<connect gate="G$1" pin="OUT4" pad="12"/>
<connect gate="G$1" pin="SNS1" pad="3"/>
<connect gate="G$1" pin="SNS1K" pad="4"/>
<connect gate="G$1" pin="SNS2" pad="1"/>
<connect gate="G$1" pin="SNS2K" pad="2"/>
<connect gate="G$1" pin="SNS3" pad="19"/>
<connect gate="G$1" pin="SNS3K" pad="20"/>
<connect gate="G$1" pin="SNS4" pad="17"/>
<connect gate="G$1" pin="SNS4K" pad="18"/>
<connect gate="G$1" pin="SYNC/SS" pad="9"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MMA7341L">
<gates>
<gate name="G$1" symbol="MMA7341L"/>
</gates>
<devices>
<device name="" package="LGA14">
<connects>
<connect gate="G$1" pin="!SLEEP" pad="7"/>
<connect gate="G$1" pin="GSEL" pad="10"/>
<connect gate="G$1" pin="TEST" pad="13"/>
<connect gate="G$1" pin="VDD" pad="6"/>
<connect gate="G$1" pin="VSS" pad="5"/>
<connect gate="G$1" pin="XOUT" pad="2"/>
<connect gate="G$1" pin="YOUT" pad="3"/>
<connect gate="G$1" pin="ZOUT" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TFDU4300">
<gates>
<gate name="G$1" symbol="TFDU4300"/>
</gates>
<devices>
<device name="" package="IR_TFDU4300_FOOT">
<connects>
<connect gate="G$1" pin="GND" pad="P$8"/>
<connect gate="G$1" pin="IREDA" pad="P$1"/>
<connect gate="G$1" pin="IREDC" pad="P$2"/>
<connect gate="G$1" pin="RXD" pad="P$4"/>
<connect gate="G$1" pin="SD" pad="P$5"/>
<connect gate="G$1" pin="TXD" pad="P$3"/>
<connect gate="G$1" pin="VCC" pad="P$6"/>
<connect gate="G$1" pin="VLOGIC" pad="P$7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="QT320">
<description>2-Channel charge transfer sensor IC capable of detecting near-proximity or touch.</description>
<gates>
<gate name="G$1" symbol="QT320"/>
</gates>
<devices>
<device name="" package="SOIC8">
<connects>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="7"/>
<connect gate="G$1" pin="S1A" pad="3"/>
<connect gate="G$1" pin="S1B" pad="5"/>
<connect gate="G$1" pin="S2A" pad="6"/>
<connect gate="G$1" pin="S2B" pad="2"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4893MA">
<description>1 Watt Audio Power Amplifier</description>
<gates>
<gate name="G$1" symbol="LM4893"/>
</gates>
<devices>
<device name="" package="SOIC8">
<connects>
<connect gate="G$1" pin="!SHUT" pad="1"/>
<connect gate="G$1" pin="BYPASS" pad="2"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="4"/>
<connect gate="G$1" pin="VDD" pad="6"/>
<connect gate="G$1" pin="VO1" pad="5"/>
<connect gate="G$1" pin="VO2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA344">
<description>LOW POWER, SINGLE-SUPPLY, RAIL-TO-RAIL
OPERATIONAL AMPLIFIERS</description>
<gates>
<gate name="G$1" symbol="OPAMP+-"/>
</gates>
<devices>
<device name="" package="SOIC8">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC2630HSC6-LZ12">
<gates>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC2630">
<gates>
<gate name="G$1" symbol="LTC2630"/>
</gates>
<devices>
<device name="" package="SC70-6">
<connects>
<connect gate="G$1" pin="!CS/LD" pad="1"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="SDI" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BLABLA_OPA344">
<description>BLABLABLALABL</description>
<gates>
<gate name="G$1" symbol="OPAMP+-"/>
</gates>
<devices>
<device name="" package="SOIC8">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MICRF0XX">
<description>The MICRF002 is a single chip ASK/OOK (ON-OFF
Keyed) RF receiver IC.</description>
<gates>
<gate name="G$1" symbol="MICRF0XX"/>
</gates>
<devices>
<device name="" package="SOIC16">
<connects>
<connect gate="G$1" pin="ANT" pad="4"/>
<connect gate="G$1" pin="CAGC" pad="13"/>
<connect gate="G$1" pin="CTH" pad="7"/>
<connect gate="G$1" pin="DO" pad="10"/>
<connect gate="G$1" pin="NC" pad="8"/>
<connect gate="G$1" pin="REFOSC" pad="15"/>
<connect gate="G$1" pin="SEL0" pad="1"/>
<connect gate="G$1" pin="SEL1" pad="14"/>
<connect gate="G$1" pin="SHUT" pad="11"/>
<connect gate="G$1" pin="SWEN" pad="16"/>
<connect gate="G$1" pin="VDDBB" pad="6"/>
<connect gate="G$1" pin="VDDRF" pad="5"/>
<connect gate="G$1" pin="VSSBB" pad="9"/>
<connect gate="G$1" pin="VSSRF1" pad="2"/>
<connect gate="G$1" pin="VSSRF2" pad="3"/>
<connect gate="G$1" pin="WAKEB" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN75178BP">
<description>The SN75178B is a differential bus repeaters RS485/RS422.</description>
<gates>
<gate name="G$1" symbol="SN75178"/>
</gates>
<devices>
<device name="" package="DIP08">
<connects>
<connect gate="G$1" pin="!EN" pad="3"/>
<connect gate="G$1" pin="A" pad="8"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="T" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="Y" pad="5"/>
<connect gate="G$1" pin="Z" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN75176AP">
<description>The SN75176A is differential bus transceiver RS422.</description>
<gates>
<gate name="G$1" symbol="SN75176A"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="!RE" pad="2"/>
<connect gate="G$1" pin="A" pad="6"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="D" pad="4"/>
<connect gate="G$1" pin="DE" pad="3"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="R" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN7517AD">
<description>The SN75176A differential bus transceiver RS422.</description>
<gates>
<gate name="G$1" symbol="SN75176A"/>
</gates>
<devices>
<device name="" package="SOIC8">
<connects>
<connect gate="G$1" pin="!RE" pad="2"/>
<connect gate="G$1" pin="A" pad="6"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="D" pad="4"/>
<connect gate="G$1" pin="DE" pad="3"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="R" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN75176BP">
<description>The SN75176B and SN65176B are differential bus transceivers RS485/RS422.</description>
<gates>
<gate name="G$1" symbol="SN75176A"/>
</gates>
<devices>
<device name="" package="DIP08">
<connects>
<connect gate="G$1" pin="!RE" pad="2"/>
<connect gate="G$1" pin="A" pad="6"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="D" pad="4"/>
<connect gate="G$1" pin="DE" pad="3"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="R" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN7517BD">
<description>The SN75176B and SN65176B are differential bus transceivers RS485/RS422.</description>
<gates>
<gate name="G$1" symbol="SN75176A"/>
</gates>
<devices>
<device name="" package="SOIC8">
<connects>
<connect gate="G$1" pin="!RE" pad="2"/>
<connect gate="G$1" pin="A" pad="6"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="D" pad="4"/>
<connect gate="G$1" pin="DE" pad="3"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="R" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM380N-8">
<description>The LM380 is a power audio amplifier for consumer applications.</description>
<gates>
<gate name="G$1" symbol="LM380N-8"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="+" pad="3"/>
<connect gate="G$1" pin="-" pad="2"/>
<connect gate="G$1" pin="BP" pad="8"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND1" pad="5"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="6"/>
<connect gate="G$1" pin="VS" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP4921">
<gates>
<gate name="G$1" symbol="MCP4921"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="!CS" pad="2"/>
<connect gate="G$1" pin="!LDAC" pad="5"/>
<connect gate="G$1" pin="AVSS" pad="7"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="SDI" pad="4"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="8"/>
<connect gate="G$1" pin="VREF" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SN" package="SOIC8">
<connects>
<connect gate="G$1" pin="!CS" pad="2"/>
<connect gate="G$1" pin="!LDAC" pad="5"/>
<connect gate="G$1" pin="AVSS" pad="7"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="SDI" pad="4"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="8"/>
<connect gate="G$1" pin="VREF" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP120">
<gates>
<gate name="G$1" symbol="MCP120/130"/>
</gates>
<devices>
<device name="TO92-D" package="TO92">
<connects>
<connect gate="G$1" pin="!RST" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VDD" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO92-G" package="TO92">
<connects>
<connect gate="G$1" pin="!RST" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VDD" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO92-H" package="TO92">
<connects>
<connect gate="G$1" pin="!RST" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VDD" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT-23-3" package="SOT23">
<connects>
<connect gate="G$1" pin="!RST" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VDD" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED_RGB_7.6MM">
<gates>
<gate name="G$1" symbol="LED_RGB"/>
</gates>
<devices>
<device name="" package="LED_TH_7.6MM">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POT_TYCO">
<gates>
<gate name="G$1" symbol="POT"/>
</gates>
<devices>
<device name="S51" package="POT_TYCO_S50">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74HCT32N">
<gates>
<gate name="G$1" symbol="74HCT32N"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="1A" pad="1"/>
<connect gate="G$1" pin="1B" pad="2"/>
<connect gate="G$1" pin="1Y" pad="3"/>
<connect gate="G$1" pin="2A" pad="4"/>
<connect gate="G$1" pin="2B" pad="5"/>
<connect gate="G$1" pin="2Y" pad="6"/>
<connect gate="G$1" pin="3A" pad="9"/>
<connect gate="G$1" pin="3B" pad="10"/>
<connect gate="G$1" pin="3Y" pad="8"/>
<connect gate="G$1" pin="4A" pad="12"/>
<connect gate="G$1" pin="4B" pad="13"/>
<connect gate="G$1" pin="4Y" pad="11"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BD622XFP">
<description>Full H-bridge driver - 2 channel - PWM control</description>
<gates>
<gate name="G$1" symbol="BD622XFP"/>
<gate name="G$2" symbol="GND"/>
<gate name="G$3" symbol="GND"/>
</gates>
<devices>
<device name="BD622XFP-HSOP25" package="HSOP25">
<connects>
<connect gate="G$1" pin="FINA" pad="11"/>
<connect gate="G$1" pin="FINB" pad="23"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="GND@2" pad="20"/>
<connect gate="G$1" pin="OUT1A" pad="1"/>
<connect gate="G$1" pin="OUT1B" pad="14"/>
<connect gate="G$1" pin="OUT2A" pad="6"/>
<connect gate="G$1" pin="OUT2B" pad="19"/>
<connect gate="G$1" pin="RINA" pad="10"/>
<connect gate="G$1" pin="RINB" pad="22"/>
<connect gate="G$1" pin="RNFA" pad="3"/>
<connect gate="G$1" pin="RNFB" pad="16"/>
<connect gate="G$1" pin="VCC@1" pad="12"/>
<connect gate="G$1" pin="VCC@2" pad="13"/>
<connect gate="G$1" pin="VCC@3" pad="24"/>
<connect gate="G$1" pin="VCC@4" pad="25"/>
<connect gate="G$1" pin="VREFA" pad="9"/>
<connect gate="G$1" pin="VREFB" pad="21"/>
<connect gate="G$2" pin="GND" pad="GND@1"/>
<connect gate="G$3" pin="GND" pad="GND@2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN74LVC1G315">
<description>This single-pole, double-throw (SPDT) analog switch is designed for 1.65-V to 5.5-V V CC operation.

The SN74LVC1G3157 can handle both analog and digital signals. The device permits signals with amplitudes of

up to V CC (peak) to be transmitted in either direction.

Applications include signal gating, chopping, modulation or demodulation (modem), and signal multiplexing for

analog-to-digital and digital-to-analog conversion systems.</description>
<gates>
<gate name="G$1" symbol="SWITCH-SPDT"/>
<gate name="G$2" symbol="VCC2"/>
<gate name="G$3" symbol="GND"/>
</gates>
<devices>
<device name="DBV" package="SOT23-6">
<connects>
<connect gate="G$1" pin="INA" pad="1"/>
<connect gate="G$1" pin="INB" pad="3"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="S" pad="6"/>
<connect gate="G$2" pin="VCC" pad="5"/>
<connect gate="G$3" pin="GND" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VCC" prefix="P+">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="VCC2"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2904">
<description>Low power dual operational amplifier.</description>
<gates>
<gate name="G$1" symbol="DUAL-OPAMP+-"/>
<gate name="G$2" symbol="PWR+GND"/>
</gates>
<devices>
<device name="D" package="SOIC8">
<connects>
<connect gate="G$1" pin="+INA" pad="3"/>
<connect gate="G$1" pin="+INB" pad="5"/>
<connect gate="G$1" pin="-INA" pad="2"/>
<connect gate="G$1" pin="-INB" pad="6"/>
<connect gate="G$1" pin="OUTA" pad="1"/>
<connect gate="G$1" pin="OUTB" pad="7"/>
<connect gate="G$2" pin="GND" pad="4"/>
<connect gate="G$2" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LD1117X">
<description>Adjustable and fixed low drop positive voltage regulator</description>
<gates>
<gate name="G$1" symbol="VREG-3PINS"/>
<gate name="G$2" symbol="GND"/>
</gates>
<devices>
<device name="S50TR" package="SOT223">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$2" pin="GND" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM386">
<description>The LM386 is a power amplifier designed for use in low voltage
consumer applications.</description>
<gates>
<gate name="G$1" symbol="OPAMP+-8"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="BYPASS" pad="7"/>
<connect gate="G$1" pin="G1" pad="1"/>
<connect gate="G$1" pin="G2" pad="8"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="V+" pad="6"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M" package="SOIC8">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="BYPASS" pad="7"/>
<connect gate="G$1" pin="G1" pad="1"/>
<connect gate="G$1" pin="G2" pad="8"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="V+" pad="6"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRIMPOT_PTH">
<description>Trim potentiometer</description>
<gates>
<gate name="G$1" symbol="POT"/>
</gates>
<devices>
<device name="" package="PINH1X03">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP73831">
<description>The MCP73831 is a highly advanced linear charge
management controller for use in space-limited, cost
sensitive applications</description>
<gates>
<gate name="G$1" symbol="MCP73831"/>
</gates>
<devices>
<device name="" package="SOT25">
<connects>
<connect gate="G$1" pin="PROG" pad="5"/>
<connect gate="G$1" pin="STAT" pad="1"/>
<connect gate="G$1" pin="VBAT" pad="3"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC3407">
<description>The LTC®
3407 is a dual, constant frequency, synchronous 
step down DC/DC converter.</description>
<gates>
<gate name="G$1" symbol="LTC3407"/>
</gates>
<devices>
<device name="" package="MSOP10">
<connects>
<connect gate="G$1" pin="!RESET" pad="8"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="MODE" pad="6"/>
<connect gate="G$1" pin="RUN1" pad="2"/>
<connect gate="G$1" pin="RUN2" pad="9"/>
<connect gate="G$1" pin="SW1" pad="4"/>
<connect gate="G$1" pin="SW2" pad="7"/>
<connect gate="G$1" pin="VFB1" pad="1"/>
<connect gate="G$1" pin="VFB2" pad="10"/>
<connect gate="G$1" pin="VIN" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP1640">
<description>The MCP1640/B/C/D is a compact, high-efficiency,
fixed frequency, synchronous step-up DC-DC converter. It provides an easy-to-use power supply solution
for applications powered by either one-cell, two-cell, or
three-cell alkaline, NiCd, NiMH, one-cell Li-Ion or
Li-Polymer batteries.</description>
<gates>
<gate name="G$1" symbol="MCP1640"/>
</gates>
<devices>
<device name="" package="SOT23-6">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SW" pad="1"/>
<connect gate="G$1" pin="VFB" pad="4"/>
<connect gate="G$1" pin="VIN" pad="6"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CIID-LABS">
<description>made by labs.ciid.dk</description>
<gates>
<gate name="G$1" symbol="CIID-LABS"/>
</gates>
<devices>
<device name="2CM" package="CIID-LABS-LOGO">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1.2CM" package="CIID-LABS-LOGO-SMALL">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BODYSWITCH">
<gates>
<gate name="G$1" symbol="BODYSWITCH"/>
</gates>
<devices>
<device name="" package="BODYSWITCH">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VSIONHAIR">
<description>VSIONHAIRIES</description>
<gates>
<gate name="G$1" symbol="VSIONHAIR"/>
<gate name="G$2" symbol="VSIONHAIR"/>
</gates>
<devices>
<device name="" package="VSIONHAIR">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
