32K flash program memory 8-bit bytes
8K/sec = 4 seconds

use 20K ?

granular synthesis is like wave-table synthesis but with playing only a selection and windowing it
the stored wave-table could be a piece of bird-call and you could play a piece by feeling it - i.e. create a "haptic-landscape" that let's you feel what part of the wave you are on.